,Reflector Diameter##other##,Enclosure Type##other##,Reflector##other##,Lamp##other##,Ballast##other##,Voltage##other##,Photometric Web File##other##
EPLB-16-O-HL-AO-XX-100L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-100L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-100L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-100L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-100L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-100L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-100L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-100L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-100L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-100L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-100L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-100L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-100L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-100L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-100L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-100L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-100L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-100L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-100L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-100L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-100L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-100L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-100L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-100L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-100L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-100L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-100L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-100L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-100L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-100L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-100L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-100L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-100L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-100L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-100L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-100L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-100L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-100L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-100L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-100L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-100L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-100L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-100L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-100L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-100L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-100L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-100L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-100L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-100L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-100L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-100L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-100L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-100L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-100L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-100L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-100L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-100L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-100L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-100L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-100L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-100L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-100L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-100L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-100L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-100L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-100L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-100L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-100L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-100L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-100L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-100L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-100L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-100L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-100L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-100L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-100L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-100L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-100L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-100L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-100L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-100L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-100L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-100L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-100L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-100L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-100L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-100L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-100L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-100L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-100L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-100L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-100L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-100L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-100L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-100L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-100L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,100 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-108L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-108L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-108L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-108L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-108L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-108L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-108L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-108L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-108L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-108L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-108L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-108L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-108L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-108L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-108L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-108L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-108L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-108L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-108L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-108L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-108L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-108L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-108L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-108L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-108L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-108L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-108L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-108L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-108L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-108L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-108L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-108L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-108L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-108L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-108L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-108L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-108L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-108L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-108L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-108L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-108L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-108L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-108L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-108L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-108L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-108L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-108L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-108L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-108L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-108L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-108L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-108L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-108L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-108L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-108L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-108L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-108L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-108L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-108L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-108L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-108L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-108L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-108L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-108L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-108L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-108L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-108L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-108L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-108L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-108L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-108L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-108L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-108L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-108L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-108L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-108L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-108L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-108L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-108L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-108L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-108L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-108L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-108L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-108L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-108L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-108L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-108L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-108L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-108L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-108L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-108L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-108L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-108L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-108L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-108L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-108L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,108 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-160L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-160L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-160L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-160L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-160L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-160L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-160L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-160L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-160L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-160L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-160L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-160L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-160L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-160L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-160L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-160L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-160L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-160L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-160L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-160L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-160L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-160L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-160L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-160L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-160L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-160L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-160L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-160L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-160L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-160L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-160L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-160L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-160L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-160L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-160L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-160L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-160L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-160L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-160L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-160L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-160L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-160L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-160L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-160L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-160L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-160L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-160L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-160L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-160L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-160L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-160L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-160L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-160L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-160L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-160L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-160L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-160L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-160L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-160L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-160L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-160L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-160L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-160L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-160L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-160L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-160L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-160L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-160L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-160L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-160L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-160L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-160L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-160L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-160L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-160L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-160L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-160L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-160L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-160L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-160L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-160L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-160L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-160L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-160L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-160L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-160L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-160L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-160L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-160L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-160L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-160L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-160L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-160L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-160L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-160L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-160L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,160 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-216L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-216L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-216L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-216L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-216L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-216L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-216L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-216L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-AO-XX-216L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-216L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-AO-XX-216L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-AO-XX-216L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-216L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-216L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-216L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-216L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-216L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-216L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-216L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-216L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CA-XX-216L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-216L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CA-XX-216L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CA-XX-216L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-216L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-216L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-216L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-216L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-216L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-216L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-216L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-216L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-PPA-XX-216L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-216L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-PPA-XX-216L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-PPA-XX-216L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-216L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-216L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-216L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-216L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-216L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-216L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-216L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-216L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-HL-CP-XX-216L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-216L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-HL-CP-XX-216L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-HL-CP-XX-216L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-216L40K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-216L40K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-216L40K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-216L40K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-216L50K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-216L50K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-216L50K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-216L50K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-AO-XX-216L57K-DCC-120,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-216L57K-DCC-277,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-AO-XX-216L57K-DCC-DV,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-AO-XX-216L57K-DCC-347,16 INCH,Dry Location,Open Aluminum Reflector,216 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-216L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-216L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-216L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-216L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-216L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-216L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-216L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-216L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CA-XX-216L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-216L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CA-XX-216L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CA-XX-216L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-216L40K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-216L40K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-216L40K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-216L40K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-216L50K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-216L50K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-216L50K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-216L50K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-PPA-XX-216L57K-DCC-120,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-216L57K-DCC-277,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-PPA-XX-216L57K-DCC-DV,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-PPA-XX-216L57K-DCC-347,16 INCH,Dry Location,Pearlescent Prismatic Acrylic,216 Watt 5700K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-216L40K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-216L40K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-216L40K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-216L40K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 4000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-216L50K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-216L50K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-216L50K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-216L50K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5000K LED,Dimming Constant Current,347,
EPLB-16-O-PM-CP-XX-216L57K-DCC-120,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-216L57K-DCC-277,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,277,
EPLB-16-O-PM-CP-XX-216L57K-DCC-DV,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,120,
EPLB-16-O-PM-CP-XX-216L57K-DCC-347,16 INCH,Dry Location,Clear Prismatic Polycarbonate,216 Watt 5700K LED,Dimming Constant Current,347,
