,Reflector Diameter##other##,Enclosure Type##other##,Reflector##other##,Lamp##other##,Ballast##other##,Voltage##other##,Photometric Web File##other##
EPLB-12-O-HL-AO-XX-26L40K-DCC-120,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-AO-XX-26L40K-DCC-277,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-AO-XX-26L40K-DCC-DV,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-AO-XX-26L40K-DCC-347,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-AO-XX-26L50K-DCC-120,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-AO-XX-26L50K-DCC-277,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-AO-XX-26L50K-DCC-DV,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-AO-XX-26L50K-DCC-347,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-AO-XX-26L57K-DCC-120,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-AO-XX-26L57K-DCC-277,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-HL-AO-XX-26L57K-DCC-DV,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-AO-XX-26L57K-DCC-347,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,347,
EPLB-12-O-HL-CA-XX-26L40K-DCC-120,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CA-XX-26L40K-DCC-277,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-CA-XX-26L40K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CA-XX-26L40K-DCC-347,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-CA-XX-26L50K-DCC-120,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CA-XX-26L50K-DCC-277,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-CA-XX-26L50K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CA-XX-26L50K-DCC-347,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-CA-XX-26L57K-DCC-120,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CA-XX-26L57K-DCC-277,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-HL-CA-XX-26L57K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CA-XX-26L57K-DCC-347,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,347,
EPLB-12-O-HL-PPA-XX-26L40K-DCC-120,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-PPA-XX-26L40K-DCC-277,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-PPA-XX-26L40K-DCC-DV,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-PPA-XX-26L40K-DCC-347,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-PPA-XX-26L50K-DCC-120,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-PPA-XX-26L50K-DCC-277,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-PPA-XX-26L50K-DCC-DV,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-PPA-XX-26L50K-DCC-347,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-PPA-XX-26L57K-DCC-120,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-PPA-XX-26L57K-DCC-277,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-HL-PPA-XX-26L57K-DCC-DV,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-PPA-XX-26L57K-DCC-347,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,347,
EPLB-12-O-HL-CP-XX-26L40K-DCC-120,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CP-XX-26L40K-DCC-277,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-CP-XX-26L40K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CP-XX-26L40K-DCC-347,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-CP-XX-26L50K-DCC-120,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CP-XX-26L50K-DCC-277,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-HL-CP-XX-26L50K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CP-XX-26L50K-DCC-347,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-HL-CP-XX-26L57K-DCC-120,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CP-XX-26L57K-DCC-277,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-HL-CP-XX-26L57K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-HL-CP-XX-26L57K-DCC-347,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,347,
EPLB-12-O-PM-AO-XX-26L40K-DCC-120,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-AO-XX-26L40K-DCC-277,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-AO-XX-26L40K-DCC-DV,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-AO-XX-26L40K-DCC-347,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-AO-XX-26L50K-DCC-120,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-AO-XX-26L50K-DCC-277,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-AO-XX-26L50K-DCC-DV,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-AO-XX-26L50K-DCC-347,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-AO-XX-26L57K-DCC-120,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-AO-XX-26L57K-DCC-277,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-PM-AO-XX-26L57K-DCC-DV,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-AO-XX-26L57K-DCC-347,12 INCH,Dry Location,Open Aluminum Reflector,26 Watt 5700K LED,Dimming Constant Current,347,
EPLB-12-O-PM-CA-XX-26L40K-DCC-120,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CA-XX-26L40K-DCC-277,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-CA-XX-26L40K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CA-XX-26L40K-DCC-347,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-CA-XX-26L50K-DCC-120,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CA-XX-26L50K-DCC-277,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-CA-XX-26L50K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CA-XX-26L50K-DCC-347,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-CA-XX-26L57K-DCC-120,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CA-XX-26L57K-DCC-277,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-PM-CA-XX-26L57K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CA-XX-26L57K-DCC-347,12 INCH,Dry Location,Clear Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,347,
EPLB-12-O-PM-PPA-XX-26L40K-DCC-120,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-PPA-XX-26L40K-DCC-277,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-PPA-XX-26L40K-DCC-DV,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-PPA-XX-26L40K-DCC-347,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-PPA-XX-26L50K-DCC-120,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-PPA-XX-26L50K-DCC-277,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-PPA-XX-26L50K-DCC-DV,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-PPA-XX-26L50K-DCC-347,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-PPA-XX-26L57K-DCC-120,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-PPA-XX-26L57K-DCC-277,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-PM-PPA-XX-26L57K-DCC-DV,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-PPA-XX-26L57K-DCC-347,12 INCH,Dry Location,Pearlescent Prismatic Acrylic,26 Watt 5700K LED,Dimming Constant Current,347,
EPLB-12-O-PM-CP-XX-26L40K-DCC-120,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CP-XX-26L40K-DCC-277,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-CP-XX-26L40K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CP-XX-26L40K-DCC-347,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 4000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-CP-XX-26L50K-DCC-120,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CP-XX-26L50K-DCC-277,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,277,
EPLB-12-O-PM-CP-XX-26L50K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CP-XX-26L50K-DCC-347,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5000K LED,Dimming Constant Current,347,
EPLB-12-O-PM-CP-XX-26L57K-DCC-120,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CP-XX-26L57K-DCC-277,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,277,
EPLB-12-O-PM-CP-XX-26L57K-DCC-DV,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,120,
EPLB-12-O-PM-CP-XX-26L57K-DCC-347,12 INCH,Dry Location,Clear Prismatic Polycarbonate,26 Watt 5700K LED,Dimming Constant Current,347,
